# $language = "VBScript"
# $interface = "1.0"
Sub Command(comm)
	crt.screen.send comm & chr(13)
	crt.screen.WaitForString "#"
End Sub
Sub Command1(comm)
	crt.screen.send comm & chr(13)
	crt.screen.WaitForString ">"
End Sub
Sub Main
crt.Screen.Synchronous = False



        Command "enable"
        Command "terminal length 0"
        Command "!无线产品信息收集开始"
        Command "show version"
	crt.sleep 1000
        Command "show version all"
	crt.sleep 1000
        Command "show version slot"
	crt.sleep 1000
        Command "show run | begin line vty"
	crt.sleep 1000
        Command "show run"
	crt.sleep 1000
        Command "more config.text"
	crt.sleep 1000
        Command "show ap-config run"
	crt.sleep 1000
        Command "show ap-config summary"
	crt.sleep 1000
        Command "show debugging"
	crt.sleep 1000
        Command "show ip dhcp pool"
	crt.sleep 1000
        Command "show ip dhcp snooping"
	crt.sleep 1000
        Command "show ip dhcp binding"
	crt.sleep 1000
        Command "debug su"
	crt.sleep 1000
        Command "show exception"
	crt.sleep 1000
        Command "show pool"
	crt.sleep 1000
        Command "show skbuff"
	crt.sleep 1000
        Command "show skbuff"
	crt.sleep 1000
        Command "show skbuff"
	crt.sleep 1000
        Command "show skbuff"
	crt.sleep 1000
        Command "show skbuff"
	crt.sleep 1000
        Command "show queue"
	crt.sleep 1000
        Command "exec ef_rwc_db"
	crt.sleep 1000
        Command "exec ef_acl_ace"
	crt.sleep 1000
        Command "exit"
	crt.sleep 1000
        Command "dir"
	crt.sleep 1000
        Command "show capwap state"
	crt.sleep 1000
        Command "show arp"
	crt.sleep 1000
        Command "show arp count"
	crt.sleep 1000
        Command "show proxy_arp"
	crt.sleep 1000
        Command "show logging"
	crt.sleep 1000
        Command "show wlan user"
	crt.sleep 1000
        Command "show ac-config client"
	crt.sleep 1000
        Command "show ip dhcp server statistics"
	crt.sleep 1000
        Command "show interfaces switchport"
	crt.sleep 1000
        Command "show interfaces status"
	crt.sleep 1000
        Command "show ip interface brief"
	crt.sleep 1000
        Command "show interfaces counters errors"
	crt.sleep 1000
        Command "show interfaces counters rate"
	crt.sleep 1000
        Command "show aggregatePort summary"  
	crt.sleep 1000
        Command "show clock"
	crt.sleep 1000
        Command "show mac count"
	crt.sleep 1000
        Command "show cpu"
	crt.sleep 1000
        Command "show memory"
	crt.sleep 1000
        Command "show ip route"
	crt.sleep 1000
        Command "show ip fpm statistics"
	crt.sleep 1000
        Command "show mac-address-table"
	crt.sleep 1000
        Command "show dot1x summary"
	crt.sleep 1000
        Command "show web-auth user all"
	crt.sleep 1000
        Command "show web-auth user statistics"
	crt.sleep 1000
        Command "show mobility summary"
	crt.sleep 1000
        Command "show wlan hot-backup"
	crt.sleep 1000
        Command "show cpu"
	crt.sleep 1000
        Command "show memory"
        Command "terminal no length"
        Command "!信息收集完毕"




End Sub  
