;; net8192su.inf 
;;
;; Netcore RTL8192S Wireless 802.11b/g/n USB 2.0 Network Adapter
;;
;; Copyright (C) 2008 Realtek Semiconductor Corp.
;;
;; this release is primarily for WHQL test.
;;

;FOR WIN 7

[Version]
Signature	= "$Windows NT$"
Class		= Net
ClassGUID	= {4d36e972-e325-11ce-bfc1-08002be10318}
Provider	= %Realtek%
CatalogFile.NT	= net8192su.cat		;; for WHQL certified
DriverVer = 07/15/2009,1085.3.0713.2009

[Manufacturer]
%Realtek% = Realtek,NTx86.6.1
%Corega% = Corega,NTx86.6.1
%DLink% = DLink,NTx86.6.1
%EnGenius% = EnGenius,NTx86.6.1
%Belkin% = Belkin,NTx86.6.1
%Guillemot% = Guillemot,NTx86.6.1
%Edimax% = Edimax,NTx86.6.1
%Sitecom% = Sitecom,NTx86.6.1
%Hawking% = Hawking,NTx86.6.1
%ASUSTeK% = ASUSTeK,NTx86.6.1

[ControlFlags]
;ExcludeFromSelect = USB\VID_0BDA&PID_8192&REV_0100
;ExcludeFromSelect = USB\VID_0BDA&PID_8192&REV_0200
ExcludeFromSelect = USB\VID_0BDA&PID_8171
ExcludeFromSelect = USB\VID_0BDA&PID_8172
ExcludeFromSelect = USB\VID_0BDA&PID_8173
ExcludeFromSelect = USB\VID_0BDA&PID_8174
ExcludeFromSelect = USB\VID_0BDA&PID_8712
ExcludeFromSelect = USB\VID_07AA&PID_0047
ExcludeFromSelect = USB\VID_07AA&PID_0051
ExcludeFromSelect = USB\VID_07D1&PID_3302
ExcludeFromSelect = USB\VID_07D1&PID_3300
ExcludeFromSelect = USB\VID_07D1&PID_3303
ExcludeFromSelect = USB\VID_1740&PID_9603
ExcludeFromSelect = USB\VID_1740&PID_9605
ExcludeFromSelect = USB\VID_050D&PID_815F
ExcludeFromSelect = USB\VID_06F8&PID_E031
ExcludeFromSelect = USB\VID_7392&PID_7612
ExcludeFromSelect = USB\VID_0DF6&PID_0045
ExcludeFromSelect = USB\VID_0DF6&PID_0049
ExcludeFromSelect = USB\VID_0DF6&PID_004B
ExcludeFromSelect = USB\VID_0DF6&PID_004C
ExcludeFromSelect = USB\VID_0E66&PID_0015
ExcludeFromSelect = USB\VID_0E66&PID_0016
ExcludeFromSelect = USB\VID_0B05&PID_1784

;;****************************************************************************
;; IDs for X86
;;****************************************************************************
[Realtek.NTx86.6.1]
;%RTL8192su.DeviceDesc% = RTL8192su.ndi, USB\VID_0BDA&PID_8192&REV_0100
;%RTL8192su.DeviceDesc% = RTL8192su.ndi, USB\VID_0BDA&PID_8192&REV_0200
%RTL8188su.DeviceDesc% = RTL8192su.ndi, USB\VID_0BDA&PID_8171
%RTL8191su.DeviceDesc% = RTL8192su.ndi, USB\VID_0BDA&PID_8172
%RTL8192gu.DeviceDesc% = RTL8192su.ndi, USB\VID_0BDA&PID_8173
%RTL8192su.DeviceDesc% = RTL8192su.ndi, USB\VID_0BDA&PID_8174
%RTL8712.DeviceDesc% = RTL8192su.ndi, USB\VID_0BDA&PID_8712

[Corega.NTx86.6.1]
%CG-WLUSBNM.DeviceDesc% = Corega.ndi, USB\VID_07AA&PID_0047
%CG-WLUSB300NX.DeviceDesc% = Corega.ndi, USB\VID_07AA&PID_0051

[Dlink.NTx86.6.1]
%DWA-130C2.DeviceDesc% = RTL8192su.ndi, USB\VID_07D1&PID_3302
%DWA-130E1.DeviceDesc% = RTL8192su.ndi, USB\VID_07D1&PID_3300
%DWA-131A1.DeviceDesc% = RTL8192su.ndi, USB\VID_07D1&PID_3303

[EnGenius.NTx86.6.1]
%EnGenius.DeviceDesc% = RTL8192su.ndi, USB\VID_1740&PID_9603
%EnGenius.DeviceDesc% = RTL8192su.ndi, USB\VID_1740&PID_9605

[Belkin.NTx86.6.1]
%Belkin.DeviceDesc% = RTL8192su.ndi, USB\VID_050D&PID_815F

[Guillemot.NTx86.6.1]
%Guillemot.DeviceDesc% = RTL8192su.ndi, USB\VID_06F8&PID_E031

[Edimax.NTx86.6.1]
%Edimax.DeviceDesc% = RTL8192su.ndi, USB\VID_7392&PID_7612

[Sitecom.NTx86.6.1]
%WL-353.DeviceDesc% = RTL8192su.ndi, USB\VID_0DF6&PID_0045
%WL-356.DeviceDesc% = RTL8192su.ndi, USB\VID_0DF6&PID_0049
%WL-349v3.DeviceDesc% = RTL8192su.ndi, USB\VID_0DF6&PID_004B
%WL-352v3.DeviceDesc% = RTL8192su.ndi, USB\VID_0DF6&PID_004C

[Hawking.NTx86.6.1]
%HawkingN.DeviceDesc% = RTL8192su.ndi, USB\VID_0E66&PID_0015
%HawkingG.DeviceDesc% = RTL8192su.ndi, USB\VID_0E66&PID_0016

[ASUSTeK.NTx86.6.1]
%ASUSTeK.DeviceDesc% = RTL8192su.ndi, USB\VID_0B05&PID_1784

;;****************************************************************************
;; IDs for X64
;;****************************************************************************
[Realtek.NTamd64.6.1]
;%RTL8192su.DeviceDesc% = RTL8192su.ndi, USB\VID_0BDA&PID_8192&REV_0100
;%RTL8192su.DeviceDesc% = RTL8192su.ndi, USB\VID_0BDA&PID_8192&REV_0200
%RTL8188su.DeviceDesc% = RTL8192su.ndi, USB\VID_0BDA&PID_8171
%RTL8191su.DeviceDesc% = RTL8192su.ndi, USB\VID_0BDA&PID_8172
%RTL8192gu.DeviceDesc% = RTL8192su.ndi, USB\VID_0BDA&PID_8173
%RTL8192su.DeviceDesc% = RTL8192su.ndi, USB\VID_0BDA&PID_8174
%RTL8712.DeviceDesc% = RTL8192su.ndi, USB\VID_0BDA&PID_8712

[Corega.NTamd64.6.1]
%CG-WLUSBNM.DeviceDesc% = Corega.ndi, USB\VID_07AA&PID_0047
%CG-WLUSB300NX.DeviceDesc% = Corega.ndi, USB\VID_07AA&PID_0051

[Dlink.NTamd64.6.1]
%DWA-130C2.DeviceDesc% = RTL8192su.ndi, USB\VID_07D1&PID_3302
%DWA-130E1.DeviceDesc% = RTL8192su.ndi, USB\VID_07D1&PID_3300
%DWA-131A1.DeviceDesc% = RTL8192su.ndi, USB\VID_07D1&PID_3303

[EnGenius.NTamd64.6.1]
%EnGenius.DeviceDesc% = RTL8192su.ndi, USB\VID_1740&PID_9603
%EnGenius.DeviceDesc% = RTL8192su.ndi, USB\VID_1740&PID_9605

[Belkin.NTamd64.6.1]
%Belkin.DeviceDesc% = RTL8192su.ndi, USB\VID_050D&PID_815F

[Guillemot.NTamd64.6.1]
%Guillemot.DeviceDesc% = RTL8192su.ndi, USB\VID_06F8&PID_E031

[Edimax.NTamd64.6.1]
%Edimax.DeviceDesc% = RTL8192su.ndi, USB\VID_7392&PID_7612

[Sitecom.NTamd64.6.1]
%WL-353.DeviceDesc% = RTL8192su.ndi, USB\VID_0DF6&PID_0045
%WL-356.DeviceDesc% = RTL8192su.ndi, USB\VID_0DF6&PID_0049
%WL-349v3.DeviceDesc% = RTL8192su.ndi, USB\VID_0DF6&PID_004B
%WL-352v3.DeviceDesc% = RTL8192su.ndi, USB\VID_0DF6&PID_004C

[Hawking.NTamd64.6.1]
%HawkingN.DeviceDesc% = RTL8192su.ndi, USB\VID_0E66&PID_0015
%HawkingG.DeviceDesc% = RTL8192su.ndi, USB\VID_0E66&PID_0016

[ASUSTeK.NTamd64.6.1]
%ASUSTeK.DeviceDesc% = RTL8192su.ndi, USB\VID_0B05&PID_1784

;;****************************************************************************
;; Windows 2000/XP
;;****************************************************************************
;;----------------------------------------------------------------------------
;; Realtek default installation
;;----------------------------------------------------------------------------
[RTL8192su.ndi.NT]
AddReg			= RTL8192su.os61.reg, RTL8192su.common.reg, RTLWLAN.reg
Characteristics	= 0x84
BusType			= 15 
CopyFiles		= RTL8192su.CopyFiles
*IfType			= 71            ; IF_TYPE_IEEE80211
*MediaType		= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8192su.ndi.NT.Services]
AddService		= RTL8192su, 2, RTL8192su.nt61.Service, RTL8192su.nt61.EventLog

[RTL8192su.ndi.NT.HW]
AddReg = RTL8192su_os61.vwifi.reg

;;----------------------------------------------------------------------------
;; Corega customized installation
;;----------------------------------------------------------------------------
[Corega.ndi.NT]
AddReg			= RTL8192su.os61.reg, RTL8192su.common.reg, Corega.reg
Characteristics	= 0x84
BusType			= 15 
CopyFiles		= RTL8192su.CopyFiles
*IfType			= 71            ; IF_TYPE_IEEE80211
*MediaType		= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[Corega.ndi.NT.Services]
AddService		= RTL8192su, 2, RTL8192su.nt61.Service, RTL8192su.nt61.EventLog

[Corega.ndi.NT.HW]
AddReg = RTL8192su_os61.vwifi.reg

;;****************************************************************************
;; Windows 2000/XP parameters
;;****************************************************************************
[RTL8192su.os61.reg]
HKR, Ndi\Interfaces,	UpperRange, 0, "ndis5,mdcwifi"
HKR, Ndi\Interfaces,	LowerRange, 0, "wlan, ethernet, vwifi"
HKR, Ndi,				Service,    0, "RTL8192su"

[RTL8192su.nt61.Service]
DisplayName    = %RTL8192su.DeviceDesc.DispName%
ServiceType    = 1		; %SERVICE_KERNEL_DRIVER%
StartType      = 3		; %SERRVICE_DEMAND_START%
ErrorControl   = 1		; %SERRVICE_ERROR_NORMAL%
ServiceBinary  = %12%\RTL8192su.sys
LoadOrderGroup = NDIS

[RTL8192su.nt61.EventLog]
AddReg = RTL8192su.nt61.AddEventLog.reg

[RTL8192su.nt61.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported  , 0x00010001, 7

;; Adds the VWiFi PNP filter
[RTL8192su_os61.vwifi.reg]
HKR,,"UpperFilters",0x00010000,"vwifibus"

;*******************************************************************************
; RTL8192su common paramters
;*******************************************************************************
[RTL8192su.common.reg]
HKR,,CcxRm,0,"0"

HKR,defaults,			AH_BcnIntv, 	0, "1000"
HKR,Ndi\params\AH_BcnIntv, 	default, 	0, "100"
HKR,Ndi\params\AH_BcnIntv,	ParamDesc, 	0, %AH_BCNINTV_STR%
HKR,Ndi\params\AH_BcnIntv, 	type, 		0, "int"
HKR,Ndi\params\AH_BcnIntv, 	min, 		0, "20"
HKR,Ndi\params\AH_BcnIntv, 	max, 		0, "1000"
HKR,Ndi\params\AH_BcnIntv, 	step, 		0, "1"

;;----------------------------------------------------------------------------
;; Realtek WLAN NIC parameters
;;----------------------------------------------------------------------------
[RTLWLAN.reg]
HKR,,SSID,0,""

HKR,,Channel,0,"10"

HKR,Ndi\params\Dot11dEnable,        ParamDesc,  0, %DOT11_ENABLE_STR%
HKR,Ndi\params\Dot11dEnable,        type,       0, "enum"
HKR,Ndi\params\Dot11dEnable,        default,    0, "0"
HKR,Ndi\params\Dot11dEnable\enum,   "0",        0, %DISABLE_STR%
HKR,Ndi\params\Dot11dEnable\enum,   "1",        0, %ENABLE_STR%
HKR,defaults,Dot11dEnable,0,"0"
HKR,,Dot11dEnable,0,"0"

HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, 	"8", 		0, %IEEE_802_11BGN_STR%
HKR,defaults,WirelessMode, 0, "8"
HKR,,WirelessMode, 0, "8"

;Inactive Power Save
HKR,,bInactivePs,0,"1"

HKR,,LedCtrl,0,"1"

HKR,,DefaultKeyID,,"0"
HKR,,DefaultKey0,,""
HKR,,DefaultKey1,,""
HKR,,DefaultKey2,,""
HKR,,DefaultKey3,,""

;;----------------------------------------------------------------------------
;; Corega WLAN NIC parameters
;;----------------------------------------------------------------------------
[Corega.reg]
HKR,,SSID,0,""

HKR,Ndi\params\Channel,       ParamDesc,  0, %CHANNEL_STR%
HKR,Ndi\params\Channel,       type,       0, "int"
HKR,Ndi\params\Channel,       default,    0, "1"
HKR,Ndi\params\Channel,       Min,        0, "1"
HKR,Ndi\params\Channel,       Max,        0, "13"
HKR,Ndi\params\Channel,       Step,       0, "1"
HKR,Ndi\params\Channel,       Base,       0, "10"
HKR,defaults,Channel,0,"1"
HKR,,Channel,0,"1"

HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, 	"8", 		0, %IEEE_802_11BGN_STR%
HKR,defaults,WirelessMode, 0, "8"
HKR,,WirelessMode, 0, "8"

;Inactive Power Save
HKR,,bInactivePs,0,"1"

HKR,,LedCtrl,0,"1"

HKR,,DefaultKeyID,,"0"
HKR,,DefaultKey0,,""
HKR,,DefaultKey1,,""
HKR,,DefaultKey2,,""
HKR,,DefaultKey3,,""

;*******************************************************************************
; Destination Directory
;*******************************************************************************
[RTL8192su.CopyFiles]
RTL8192su.sys,,,2

[DestinationDirs]
DefaultDestDir     = 11
RTL8192su.CopyFiles		= 12

;;****************************************************************************
;; Source Files
;;****************************************************************************
[SourceDisksFiles]
RTL8192su.sys = 1

[SourceDisksNames]
1=%DISKNAME%,,,

;*******************************************************************************
; Strings
;*******************************************************************************
[Strings]
Realtek 			= "Netcore Corp."
SSID_STR			= "SSID"
CHANNEL_STR			= "Channel"
NETWORK_TYPE_STR		= "Network Type"
LED_CONTROL_STR			= "LED Control" 
POWER_SAVE_STR			= "Power Save Mode"
WIFI_IBSS_STR			= "IBSS Default 11b Mode"
RATE_ADAPTIVE_STR		= "Rate Adaptive"
QOS_STR				= "QoS"
WMM_APSD			= "WMM APSD"
CCX_RM_STR			= "CCX Radio Measurement"
CCX_OFF_LINE_DUR_UP_LIMIT_STR	= "CCX Max Off-Line Measurement (0: unlimited)"
FORCE_PRIORITY_STR		= "Forced Priority"
HW_PARA_STR			= "Init from HwParaFile"
THREE_WIRE_MODE_STR		= "Three Wire Programming Mode"
BOARD_TYPE_STR			= "Board Type"
PROTECTION_MODE_STR		= "Protection Mode"
TPC_STR				= "Transmit Power Control"
TPC_POLARITY_STR		= "TPC Polarity Select"
HIGH_POWER_STR			= "High Power Mechanism"
INIT_GAIN_STR			= "Initial Gain State"
CW_MAX_MIN_STR			= "Contention Window"
PSP_XLINK_STR			= "PSP XLink Mode"
CHANNEL_PLAN_STR		= "Channel Plan"
WL_MODE_STR			= "Wireless Mode"
PREAMBLE_MODE_STR		= "Preamble Mode"
FRAGTHRESH_STR			= "Fragmentation Threshold"
RTSTHRESH_STR			= "RTS Threshold"
DOT11_ENABLE_STR		= "802.11d"
Corega		                = "Allied Telesis K.K."
EnGenius			= "EnGenius Technologies"
DLink				= "D-Link Corporation"
Belkin				= "Belkin International, Inc."
Guillemot			= "Guillemot Corporation S.A"
Edimax				= "Edimax Technology Co., Ltd"
Sitecom				= "Sitecom Europe BV"
Hawking				= "Hawking Technologies, Inc."
ASUSTeK				= "ASUSTeK Computer Inc."
AH_BCNINTV_STR 			= "Beacon Interval"
DISABLE_STR 			= "Disable"
ENABLE_STR 			= "Enable"
IEEE_802_11B_STR 		= "IEEE 802.11b"
IEEE_802_11BG_STR 		= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 		= "IEEE 802.11b/g/n"

;; Source disk name
DISKNAME			= "Netcore RTL8192SU 802.11n USB 2.0无线网络适配器驱动光盘"
RTL8188su.DeviceDesc 		= "Netcore RTL8192SU 802.11n USB 2.0无线网络适配器"
RTL8188su.DeviceDesc.DispName	= "Netcore RTL8192SU 802.11n USB 2.0无线网络适配器"
RTL8191su.DeviceDesc 		= "Netcore RTL8192SU 802.11n USB 2.0无线网络适配器"
RTL8191su.DeviceDesc.DispName	= "Netcore RTL8192SU 802.11n USB 2.0无线网络适配器"
RTL8192gu.DeviceDesc 		= "Netcore RTL8192SU 802.11n USB 2.0无线网络适配器"
RTL8192gu.DeviceDesc.DispName	= "Netcore RTL8192SU 802.11n USB 2.0无线网络适配器"
RTL8192su.DeviceDesc 		= "Netcore RTL8192SU 802.11n USB 2.0无线网络适配器"
RTL8192su.DeviceDesc.DispName	= "Netcore RTL8192SU 802.11n USB 2.0无线网络适配器"
RTL8712.DeviceDesc 		= "Netcore RTL8192SU 802.11n USB 2.0无线网络适配器"
RTL8712.DeviceDesc.DispName	= "Netcore RTL8192SU 802.11n USB 2.0无线网络适配器"
CG-WLUSBNM.DeviceDesc		= "CG-WLUSBNM"
CG-WLUSBNM.DeviceDesc.DispName	= "CG-WLUSBNM"
CG-WLUSB300NX.DeviceDesc	= "CG-WLUSB300NX"
CG-WLUSB300NX.DeviceDesc.DispName= "CG-WLUSB300NX"
DWA-130C2.DeviceDesc		= "D-Link DWA-130 Wireless N USB Adapter(rev.C2)"
DWA-130C2.DeviceDesc.DispName	= "D-Link DWA-130 Wireless N USB Adapter(rev.C2)"
DWA-130E1.DeviceDesc		= "D-Link DWA-130 Wireless N USB Adapter"
DWA-130E1.DeviceDesc.DispName	= "D-Link DWA-130 Wireless N USB Adapter"
DWA-131A1.DeviceDesc		= "D-Link DWA-131 Wireless N Nano USB Adapter"
DWA-131A1.DeviceDesc.DispName	= "D-Link DWA-131 Wireless N Nano USB Adapter"
EnGenius.DeviceDesc		= "EnGenius 802.11n Wireless USB Adapter"
EnGenius.DeviceDesc.DispName	= "EnGenius 802.11n Wireless USB Adapter"
Belkin.DeviceDesc		= "Belkin N Wireless USB Adapter"
Belkin.DeviceDesc.DispName	= "Belkin N Wireless USB Adapter"
Guillemot.DeviceDesc		= "Hercules Wireless N Mini USB Key"
Guillemot.DeviceDesc.DispName	= "Hercules Wireless N Mini USB Key"
Edimax.DeviceDesc		= "Edimax 802.11n Wireless USB Adapter"
Edimax.DeviceDesc.DispName	= "Edimax 802.11n Wireless USB Adapter"
WL-353.DeviceDesc		= "Sitecom Wireless Nano USB Adapter 150N WL-353"
WL-353.DeviceDesc.DispName	= "Sitecom Wireless Nano USB Adapter 150N WL-353"
WL-356.DeviceDesc		= "Sitecom Wireless High-Gain USB Adapter 300N X2 WL-356"
WL-356.DeviceDesc.DispName	= "Sitecom Wireless High-Gain USB Adapter 300N X2 WL-356"
WL-349v3.DeviceDesc		= "Sitecom 150N Wireless USB adapter WL-349v3"
WL-349v3.DeviceDesc.DispName	= "Sitecom 150N Wireless USB adapter WL-349v3"
WL-352v3.DeviceDesc		= "Sitecom 300N Wireless USB Adapter WL-352v3"
WL-352v3.DeviceDesc.DispName	= "Sitecom 300N Wireless USB Adapter WL-352v3"
HawkingN.DeviceDesc		= "Hawking Hi-Gain USB Wireless-N Dish Adapter"
HawkingN.DeviceDesc.DispName	= "Hawking Hi-Gain USB Wireless-N Dish Adapter"
HawkingG.DeviceDesc		= "Hawking Hi-Gain USB Wireless-G Dish Adapter"
HawkingG.DeviceDesc.DispName	= "Hawking Hi-Gain USB Wireless-G Dish Adapter"
ASUSTeK.DeviceDesc		= "ASUS SuperSpeed N Wireless Adapter"
ASUSTeK.DeviceDesc.DispName	= "ASUS SuperSpeed N Wireless Adapter"