
## INIFILEVERSION #############################################################

[INIFILEVERSION]
VERSION		= 200

## GENERAL ####################################################################

[GENERAL]
DESCRIPTION	= ISO Turning
BASICTYPE	= 0
PRINTCOL	= 2
COLINDICATOR	= 60
HIDEASSIST	= No
LOADORDER	= 2

## RENUM ######################################################################

[RENUM]
AUTOINDENT	= Yes
UNDOLARGE	= No
INSERTSPACE	= 1
STARTNEXT	= No
RENUMEMPTY	= No
SHOWQUICK	= No
FORMAT		= 0
INTERVAL	= 1
START		= 100
FROM		= 0
TO		= 0
RESTART		= 0
RENUMCANNED	= No
PRECEEDESTR	= N
STARTTRIG	= 
SKIP		= %,O
SKIPCONTAIN	= 

## FILECOMPARE ################################################################

[FILECOMPARE]
SINGLESTEP	= Yes
IGNORECASE	= Yes
IGNOREBLOCK	= Yes
IGNORETNUMERIC	= Yes
IGNORECOMMENTS	= Yes
IGNOREWHITESPACE= Yes
MARKCHANGEONLY	= Yes
TABSWITCH	= Yes
SMARTMARK	= Yes
AUTONEXT	= Yes
SHOWALL		= Yes

## LOADSAVE ###################################################################

[LOADSAVE]
AUTOSAVETIME	= 0
LINEFEEDTYPE	= 0
DIFFLOADSAVE	= No
REGDEFAULTEXT	= Yes
REGOTHEREXT	= Yes
SAVEEXT		= NC
LOADEXT		= NCL,ISO,NCF
LOADPATH	= 
SAVEPATH	= 

## MACHINETYPE ################################################################

[MACHINETYPE]
BLOCKSKIP	= /
COMMENTSTART	= (
COMMENTEND	= )
DECIMAL		= .
FEED		= F
SPEED		= S
TOOLCHANGE	= T
TOOLLOAD	= M6
ARCTPYE		= 0
PATHUNIT	= 0
FEEDUNIT	= 0
BLOCKSKIPAFTER	= Yes
RAPIDRATE	= 1000

## BACKPLOT ###################################################################

[BACKPLOT]
TURNPRG		= Yes
DIAPRG		= Yes
DIAARC		= No
AUTOX		= Yes
SHOWCYCLES	= Yes
NULLARCS	= Yes
PRINTQUALITY	= 2
TOOLTYPE	= 0
PRINTLOWCOLOR	= No
PRINTNOWCOLOR	= No
PLOTMODE	= 0
DRAWDIMMED	= No
SHOWTOOL	= No
SHOWRAPIDMOVES	= No
SHOWDOTS	= No
SHOWVECTORS	= No
HIGHLIGHTARCS	= No
NOPERSPECTIVE	= No
HIDEPLOTCTRL	= No
HIDECOORD	= No
TOOLDIA		= 

## CNCCALC ####################################################################

[CNCCALC]
ISTURN		= Yes
DECIMALS	= 3
TURNNEGATIVEX	= No
TURNDIAMETERPRG	= Yes
TURNDIAMETERARC	= No
ARCTYPE		= 1
GRIDON		= Yes
AXISON		= Yes
MODALXY		= Yes
MODALZ		= No
ALWAYSSIGN	= No
SHOWSUBGRID	= Yes
GRIDSIZE	= 10.000000
TRAILZEROS	= 0
METRICIMPERIAL	= 0
MACROHEAD	= 
MACROTAIL	= 
DRAWDIR		= 

## NCBASE #####################################################################

[NCBASE]
GROUPS		= 
STORE		= No
ID		= 0

## MACROINF ###################################################################

[MACROINF]
COUNT		= 81
CURRENT		= 0

## MACRO082 ###################################################################

[MACRO082]
NAME		= G94 Simple face cutting cycle
HIDEFORMULAS	= No
TEXT		= G94
PARAMCOUNT	= 0

## MACRO081 ###################################################################

[MACRO081]
NAME		= M99 Subprogram end or Macro end
HIDEFORMULAS	= No
TEXT		= M99
PARAMCOUNT	= 0

## MACRO000 ###################################################################

[MACRO000]
NAME		= Program Start and End
HIDEFORMULAS	= Yes
TEXT		= %ÿ$1ÿ(-- $2 --)ÿ(-- CIMCO START OF FILE --)ÿG21 G40ÿG54ÿG50 $3ÿÿÿÿÿ(-- CIMCO END OF FILE --)ÿM09ÿM05ÿM30ÿ%ÿ
PARAMCOUNT	= 3
000DESC		= Program number
000REQUIRED	= Yes
000ISFUNC	= No
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= No
000NOEMPTYLINE	= No
000ALLOWALPHA	= No
000REMEBER	= Yes
000DEFAULT	= 
000PREFIX	= O
000SUFFIX	= 
000MIN		= 1000
000MAX		= 6000
000DECIMALS	= 0
000DIGITS	= 0
000LASTVAL	= 1000
001DESC		= Program description
001REQUIRED	= Yes
001ISFUNC	= No
001USESIGN	= No
001UPPERCASE	= Yes
001ALLOWNEG	= Yes
001NOEMPTYLINE	= No
001ALLOWALPHA	= Yes
001REMEBER	= Yes
001DEFAULT	= 
001PREFIX	= 
001SUFFIX	= 
001MIN		= 
001MAX		= 
001DECIMALS	= -2
001DIGITS	= 0
001LASTVAL	= CIMCO
002DESC		= Max spindle speed
002REQUIRED	= Yes
002ISFUNC	= No
002USESIGN	= No
002UPPERCASE	= Yes
002ALLOWNEG	= No
002NOEMPTYLINE	= No
002ALLOWALPHA	= No
002REMEBER	= Yes
002DEFAULT	= 
002PREFIX	= S
002SUFFIX	= 
002MIN		= 
002MAX		= 
002DECIMALS	= 0
002DIGITS	= 0
002LASTVAL	= 5000

## MACRO001 ###################################################################

[MACRO001]
NAME		= Tool change with Constant Surface Speed
HIDEFORMULAS	= Yes
TEXT		= (-- $1 --)ÿ(-- CONSTANT SURFACE SPEED --)ÿ$2 @5{$2}$3ÿG18 G99ÿG96 $4 M03ÿ(-- START MOTION --)ÿÿÿ(-- END MOTION --)ÿM09ÿG28 U0. W0.ÿM01ÿ
PARAMCOUNT	= 5
000DESC		= Tool description
000REQUIRED	= Yes
000ISFUNC	= No
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= Yes
000NOEMPTYLINE	= No
000ALLOWALPHA	= Yes
000REMEBER	= Yes
000DEFAULT	= 
000PREFIX	= 
000SUFFIX	= 
000MIN		= 
000MAX		= 
000DECIMALS	= -2
000DIGITS	= 0
000LASTVAL	= 80 DEGREE ROUGHER
001DESC		= Tool number
001REQUIRED	= Yes
001ISFUNC	= No
001USESIGN	= No
001UPPERCASE	= Yes
001ALLOWNEG	= No
001NOEMPTYLINE	= No
001ALLOWALPHA	= No
001REMEBER	= No
001DEFAULT	= 
001PREFIX	= N
001SUFFIX	= 
001MIN		= 
001MAX		= 
001DECIMALS	= 0
001DIGITS	= 0
001LASTVAL	= 1
002DESC		= Tool offset number
002REQUIRED	= Yes
002ISFUNC	= No
002USESIGN	= No
002UPPERCASE	= Yes
002ALLOWNEG	= No
002NOEMPTYLINE	= No
002ALLOWALPHA	= No
002REMEBER	= No
002DEFAULT	= 
002PREFIX	= 
002SUFFIX	= 
002MIN		= 
002MAX		= 
002DECIMALS	= 0
002DIGITS	= 2
002LASTVAL	= 1
003DESC		= Constant surface speed (units/min)
003REQUIRED	= Yes
003ISFUNC	= No
003USESIGN	= No
003UPPERCASE	= Yes
003ALLOWNEG	= No
003NOEMPTYLINE	= No
003ALLOWALPHA	= No
003REMEBER	= Yes
003DEFAULT	= 
003PREFIX	= S
003SUFFIX	= 
003MIN		= 
003MAX		= 
003DECIMALS	= 0
003DIGITS	= 0
003LASTVAL	= 450
004DESC		= 
004REQUIRED	= No
004ISFUNC	= Yes
004USESIGN	= No
004UPPERCASE	= Yes
004ALLOWNEG	= No
004NOEMPTYLINE	= No
004ALLOWALPHA	= No
004REMEBER	= Yes
004DEFAULT	= 
004PREFIX	= T
004SUFFIX	= 
004MIN		= 
004MAX		= 
004DECIMALS	= 0
004DIGITS	= 2
004LASTVAL	= 01

## MACRO002 ###################################################################

[MACRO002]
NAME		= Tool change with Constant RPM
HIDEFORMULAS	= Yes
TEXT		= (-- $1 --)ÿ(-- CONSTANT RPM --)ÿ$2 @5{$2}$3ÿG18 G99ÿG97 $4 M03ÿ(-- START MOTION --)ÿÿÿ(-- END MOTION --)ÿM09ÿG28 U0. W0.ÿM01ÿ
PARAMCOUNT	= 5
000DESC		= Tool description
000REQUIRED	= Yes
000ISFUNC	= No
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= Yes
000NOEMPTYLINE	= No
000ALLOWALPHA	= Yes
000REMEBER	= Yes
000DEFAULT	= 
000PREFIX	= 
000SUFFIX	= 
000MIN		= 
000MAX		= 
000DECIMALS	= -2
000DIGITS	= 0
000LASTVAL	= CUTOFF
001DESC		= Tool number
001REQUIRED	= Yes
001ISFUNC	= No
001USESIGN	= No
001UPPERCASE	= Yes
001ALLOWNEG	= No
001NOEMPTYLINE	= No
001ALLOWALPHA	= No
001REMEBER	= No
001DEFAULT	= 
001PREFIX	= N
001SUFFIX	= 
001MIN		= 
001MAX		= 
001DECIMALS	= 0
001DIGITS	= 0
001LASTVAL	= 2
002DESC		= Tool offset number
002REQUIRED	= Yes
002ISFUNC	= No
002USESIGN	= No
002UPPERCASE	= Yes
002ALLOWNEG	= No
002NOEMPTYLINE	= No
002ALLOWALPHA	= No
002REMEBER	= No
002DEFAULT	= 
002PREFIX	= 
002SUFFIX	= 
002MIN		= 
002MAX		= 
002DECIMALS	= 0
002DIGITS	= 2
002LASTVAL	= 2
003DESC		= Spindle Speed (rev/min)
003REQUIRED	= Yes
003ISFUNC	= No
003USESIGN	= No
003UPPERCASE	= Yes
003ALLOWNEG	= No
003NOEMPTYLINE	= No
003ALLOWALPHA	= No
003REMEBER	= Yes
003DEFAULT	= 
003PREFIX	= S
003SUFFIX	= 
003MIN		= 
003MAX		= 
003DECIMALS	= 0
003DIGITS	= 0
003LASTVAL	= 2000
004DESC		= 
004REQUIRED	= No
004ISFUNC	= Yes
004USESIGN	= No
004UPPERCASE	= Yes
004ALLOWNEG	= Yes
004NOEMPTYLINE	= No
004ALLOWALPHA	= No
004REMEBER	= Yes
004DEFAULT	= 
004PREFIX	= T
004SUFFIX	= 
004MIN		= 
004MAX		= 
004DECIMALS	= 0
004DIGITS	= 2
004LASTVAL	= 02

## MACRO003 ###################################################################

[MACRO003]
NAME		= Program comment
HIDEFORMULAS	= No
TEXT		= (-- $1 --)
PARAMCOUNT	= 1
000DESC		= Program comment
000REQUIRED	= Yes
000ISFUNC	= No
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= Yes
000NOEMPTYLINE	= No
000ALLOWALPHA	= Yes
000REMEBER	= Yes
000DEFAULT	= 
000PREFIX	= 
000SUFFIX	= 
000MIN		= 
000MAX		= 
000DECIMALS	= -2
000DIGITS	= 0
000LASTVAL	= TOOL CHANGE

## MACRO004 ###################################################################

[MACRO004]
NAME		= G00 Rapid move
HIDEFORMULAS	= No
TEXT		= G00 $1 $2
PARAMCOUNT	= 2
000DESC		= X coordinate
000REQUIRED	= No
000ISFUNC	= No
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= Yes
000NOEMPTYLINE	= No
000ALLOWALPHA	= No
000REMEBER	= No
000DEFAULT	= 
000PREFIX	= X
000SUFFIX	= 
000MIN		= 
000MAX		= 
000DECIMALS	= -1
000DIGITS	= 0
000LASTVAL	= 
001DESC		= Z coordinate
001REQUIRED	= No
001ISFUNC	= No
001USESIGN	= No
001UPPERCASE	= Yes
001ALLOWNEG	= Yes
001NOEMPTYLINE	= No
001ALLOWALPHA	= No
001REMEBER	= No
001DEFAULT	= 
001PREFIX	= Z
001SUFFIX	= 
001MIN		= 
001MAX		= 
001DECIMALS	= -1
001DIGITS	= 0
001LASTVAL	= 

## MACRO005 ###################################################################

[MACRO005]
NAME		= G01 Linear move
HIDEFORMULAS	= No
TEXT		= G01 $1 $2
PARAMCOUNT	= 2
000DESC		= X coordinate
000REQUIRED	= No
000ISFUNC	= No
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= Yes
000NOEMPTYLINE	= No
000ALLOWALPHA	= No
000REMEBER	= No
000DEFAULT	= 
000PREFIX	= X
000SUFFIX	= 
000MIN		= 
000MAX		= 
000DECIMALS	= -1
000DIGITS	= 0
000LASTVAL	= 
001DESC		= Z coordinate
001REQUIRED	= No
001ISFUNC	= No
001USESIGN	= No
001UPPERCASE	= Yes
001ALLOWNEG	= Yes
001NOEMPTYLINE	= No
001ALLOWALPHA	= No
001REMEBER	= No
001DEFAULT	= 
001PREFIX	= Z
001SUFFIX	= 
001MIN		= 
001MAX		= 
001DECIMALS	= -1
001DIGITS	= 0
001LASTVAL	= 

## MACRO006 ###################################################################

[MACRO006]
NAME		= G02 Clockwise arc move
HIDEFORMULAS	= No
TEXT		= G02 $1 $2 $3
PARAMCOUNT	= 3
000DESC		= X coordinate
000REQUIRED	= No
000ISFUNC	= No
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= Yes
000NOEMPTYLINE	= No
000ALLOWALPHA	= No
000REMEBER	= No
000DEFAULT	= 
000PREFIX	= X
000SUFFIX	= 
000MIN		= 
000MAX		= 
000DECIMALS	= -1
000DIGITS	= 0
000LASTVAL	= 
001DESC		= Z coordinate
001REQUIRED	= No
001ISFUNC	= No
001USESIGN	= No
001UPPERCASE	= Yes
001ALLOWNEG	= Yes
001NOEMPTYLINE	= No
001ALLOWALPHA	= No
001REMEBER	= No
001DEFAULT	= 
001PREFIX	= Z
001SUFFIX	= 
001MIN		= 
001MAX		= 
001DECIMALS	= -1
001DIGITS	= 0
001LASTVAL	= 
002DESC		= Arc radius (set negative for arc sweep greater than 180 degrees)
002REQUIRED	= Yes
002ISFUNC	= No
002USESIGN	= No
002UPPERCASE	= Yes
002ALLOWNEG	= Yes
002NOEMPTYLINE	= No
002ALLOWALPHA	= No
002REMEBER	= Yes
002DEFAULT	= 
002PREFIX	= R
002SUFFIX	= 
002MIN		= 
002MAX		= 
002DECIMALS	= -1
002DIGITS	= 0
002LASTVAL	= 

## MACRO007 ###################################################################

[MACRO007]
NAME		= G03 Counterclockwise arc move
HIDEFORMULAS	= No
TEXT		= G03 $1 $2 $3
PARAMCOUNT	= 3
000DESC		= X coordinate
000REQUIRED	= No
000ISFUNC	= No
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= Yes
000NOEMPTYLINE	= No
000ALLOWALPHA	= No
000REMEBER	= No
000DEFAULT	= 
000PREFIX	= X
000SUFFIX	= 
000MIN		= 
000MAX		= 
000DECIMALS	= -1
000DIGITS	= 0
000LASTVAL	= 
001DESC		= Z coordinate
001REQUIRED	= No
001ISFUNC	= No
001USESIGN	= No
001UPPERCASE	= Yes
001ALLOWNEG	= Yes
001NOEMPTYLINE	= No
001ALLOWALPHA	= No
001REMEBER	= No
001DEFAULT	= 
001PREFIX	= Z
001SUFFIX	= 
001MIN		= 
001MAX		= 
001DECIMALS	= -1
001DIGITS	= 0
001LASTVAL	= 
002DESC		= Arc radius (set negative for arc sweep greater than 180 degrees)
002REQUIRED	= Yes
002ISFUNC	= No
002USESIGN	= No
002UPPERCASE	= Yes
002ALLOWNEG	= Yes
002NOEMPTYLINE	= No
002ALLOWALPHA	= No
002REMEBER	= Yes
002DEFAULT	= 
002PREFIX	= R
002SUFFIX	= 
002MIN		= 
002MAX		= 
002DECIMALS	= -1
002DIGITS	= 0
002LASTVAL	= 

## MACRO008 ###################################################################

[MACRO008]
NAME		= G04 Dwell
HIDEFORMULAS	= No
TEXT		= G04 $1
PARAMCOUNT	= 1
000DESC		= Dwell time (seconds)
000REQUIRED	= Yes
000ISFUNC	= No
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= No
000NOEMPTYLINE	= No
000ALLOWALPHA	= No
000REMEBER	= Yes
000DEFAULT	= 
000PREFIX	= X
000SUFFIX	= 
000MIN		= 
000MAX		= 
000DECIMALS	= -1
000DIGITS	= 0
000LASTVAL	= 1

## MACRO009 ###################################################################

[MACRO009]
NAME		= G10 Data setting mode
HIDEFORMULAS	= No
TEXT		= G10
PARAMCOUNT	= 0

## MACRO010 ###################################################################

[MACRO010]
NAME		= G11 Data setting mode cancel
HIDEFORMULAS	= No
TEXT		= G11
PARAMCOUNT	= 0

## MACRO011 ###################################################################

[MACRO011]
NAME		= G18 ZX plane designation
HIDEFORMULAS	= No
TEXT		= G18
PARAMCOUNT	= 0

## MACRO012 ###################################################################

[MACRO012]
NAME		= G20 Inch data input
HIDEFORMULAS	= No
TEXT		= G20
PARAMCOUNT	= 0

## MACRO013 ###################################################################

[MACRO013]
NAME		= G21 Metric data input
HIDEFORMULAS	= No
TEXT		= G21
PARAMCOUNT	= 0

## MACRO014 ###################################################################

[MACRO014]
NAME		= G27  Reference point return check
HIDEFORMULAS	= No
TEXT		= G27
PARAMCOUNT	= 0

## MACRO015 ###################################################################

[MACRO015]
NAME		= G28 Return to reference point
HIDEFORMULAS	= No
TEXT		= G28
PARAMCOUNT	= 0

## MACRO016 ###################################################################

[MACRO016]
NAME		= G29 Return from reference point
HIDEFORMULAS	= No
TEXT		= G29
PARAMCOUNT	= 0

## MACRO017 ###################################################################

[MACRO017]
NAME		= G30 Return to 2nd, 3rd and 4th reference point
HIDEFORMULAS	= No
TEXT		= G30
PARAMCOUNT	= 0

## MACRO018 ###################################################################

[MACRO018]
NAME		= G31 Skip cutting
HIDEFORMULAS	= No
TEXT		= G31
PARAMCOUNT	= 0

## MACRO019 ###################################################################

[MACRO019]
NAME		= G32 Thread cutting constant lead thread
HIDEFORMULAS	= No
TEXT		= G32
PARAMCOUNT	= 0

## MACRO020 ###################################################################

[MACRO020]
NAME		= G34 Threading function variable lead thread
HIDEFORMULAS	= No
TEXT		= G34
PARAMCOUNT	= 0

## MACRO021 ###################################################################

[MACRO021]
NAME		= G35 Circular threading CW
HIDEFORMULAS	= No
TEXT		= G35
PARAMCOUNT	= 0

## MACRO022 ###################################################################

[MACRO022]
NAME		= G36 Circular threading CCW or
HIDEFORMULAS	= No
TEXT		= G36
PARAMCOUNT	= 0

## MACRO023 ###################################################################

[MACRO023]
NAME		= G36 Automatic tool compensation X axis
HIDEFORMULAS	= No
TEXT		= G36
PARAMCOUNT	= 0

## MACRO024 ###################################################################

[MACRO024]
NAME		= G37 Automatic tool compensation Z axis
HIDEFORMULAS	= No
TEXT		= G37
PARAMCOUNT	= 0

## MACRO025 ###################################################################

[MACRO025]
NAME		= G40 Tool nose compensation cancel
HIDEFORMULAS	= No
TEXT		= G40
PARAMCOUNT	= 0

## MACRO026 ###################################################################

[MACRO026]
NAME		= G41 Tool nose compensation left
HIDEFORMULAS	= No
TEXT		= G41
PARAMCOUNT	= 0

## MACRO027 ###################################################################

[MACRO027]
NAME		= G42 Tool nose compensation right
HIDEFORMULAS	= No
TEXT		= G42
PARAMCOUNT	= 0

## MACRO028 ###################################################################

[MACRO028]
NAME		= G50 Maximum spindle speed
HIDEFORMULAS	= No
TEXT		= G50 $1
PARAMCOUNT	= 1
000DESC		= Max spindle speed
000REQUIRED	= Yes
000ISFUNC	= No
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= No
000NOEMPTYLINE	= No
000ALLOWALPHA	= No
000REMEBER	= Yes
000DEFAULT	= 3600
000PREFIX	= S
000SUFFIX	= 
000MIN		= 
000MAX		= 
000DECIMALS	= 0
000DIGITS	= 0
000LASTVAL	= 3600

## MACRO029 ###################################################################

[MACRO029]
NAME		= G52 Local coordinate system setting
HIDEFORMULAS	= No
TEXT		= G52
PARAMCOUNT	= 0

## MACRO030 ###################################################################

[MACRO030]
NAME		= G53 Machine coordinate system setting
HIDEFORMULAS	= No
TEXT		= G53
PARAMCOUNT	= 0

## MACRO031 ###################################################################

[MACRO031]
NAME		= G54 Work coordinate offset 1
HIDEFORMULAS	= No
TEXT		= G54
PARAMCOUNT	= 0

## MACRO032 ###################################################################

[MACRO032]
NAME		= G55 Work coordinate offset 2
HIDEFORMULAS	= No
TEXT		= G55
PARAMCOUNT	= 0

## MACRO033 ###################################################################

[MACRO033]
NAME		= G56 Work coordinate offset 3
HIDEFORMULAS	= No
TEXT		= G56
PARAMCOUNT	= 0

## MACRO034 ###################################################################

[MACRO034]
NAME		= G57 Work coordinate offset 4
HIDEFORMULAS	= No
TEXT		= G57
PARAMCOUNT	= 0

## MACRO035 ###################################################################

[MACRO035]
NAME		= G58 Work coordinate offset 5
HIDEFORMULAS	= No
TEXT		= G58
PARAMCOUNT	= 0

## MACRO036 ###################################################################

[MACRO036]
NAME		= G59 Work coordinate offset 6
HIDEFORMULAS	= No
TEXT		= G59
PARAMCOUNT	= 0

## MACRO037 ###################################################################

[MACRO037]
NAME		= G61 Exact stop mode
HIDEFORMULAS	= No
TEXT		= G61
PARAMCOUNT	= 0

## MACRO038 ###################################################################

[MACRO038]
NAME		= G62 Automatic corner override
HIDEFORMULAS	= No
TEXT		= G62
PARAMCOUNT	= 0

## MACRO039 ###################################################################

[MACRO039]
NAME		= G64 Cutting mode
HIDEFORMULAS	= No
TEXT		= G64
PARAMCOUNT	= 0

## MACRO040 ###################################################################

[MACRO040]
NAME		= G65 Custom macro call
HIDEFORMULAS	= No
TEXT		= G65
PARAMCOUNT	= 0

## MACRO041 ###################################################################

[MACRO041]
NAME		= G66 Custom macro call modal
HIDEFORMULAS	= No
TEXT		= G66
PARAMCOUNT	= 0

## MACRO042 ###################################################################

[MACRO042]
NAME		= G67 Custom macro call cancel
HIDEFORMULAS	= No
TEXT		= G67
PARAMCOUNT	= 0

## MACRO043 ###################################################################

[MACRO043]
NAME		= G68 Mirror image for double turrets ON
HIDEFORMULAS	= No
TEXT		= G68
PARAMCOUNT	= 0

## MACRO044 ###################################################################

[MACRO044]
NAME		= G69 Mirror image for double turrets OFF
HIDEFORMULAS	= No
TEXT		= G69
PARAMCOUNT	= 0

## MACRO045 ###################################################################

[MACRO045]
NAME		= G70 Profile finishing cycle
HIDEFORMULAS	= No
TEXT		= G70 $1 $2 $3 $4
PARAMCOUNT	= 4
000DESC		= P First block number of the finishing contour
000REQUIRED	= Yes
000ISFUNC	= No
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= No
000NOEMPTYLINE	= No
000ALLOWALPHA	= No
000REMEBER	= Yes
000DEFAULT	= 
000PREFIX	= P
000SUFFIX	= 
000MIN		= 
000MAX		= 
000DECIMALS	= 0
000DIGITS	= 0
000LASTVAL	= 100
001DESC		= Q Last block number of the finishing contour
001REQUIRED	= Yes
001ISFUNC	= No
001USESIGN	= No
001UPPERCASE	= Yes
001ALLOWNEG	= No
001NOEMPTYLINE	= No
001ALLOWALPHA	= No
001REMEBER	= Yes
001DEFAULT	= 
001PREFIX	= Q
001SUFFIX	= 
001MIN		= 
001MAX		= 
001DECIMALS	= 0
001DIGITS	= 0
001LASTVAL	= 200
002DESC		= F Cutting feedrate units/rev
002REQUIRED	= No
002ISFUNC	= No
002USESIGN	= No
002UPPERCASE	= Yes
002ALLOWNEG	= No
002NOEMPTYLINE	= No
002ALLOWALPHA	= No
002REMEBER	= Yes
002DEFAULT	= 
002PREFIX	= F
002SUFFIX	= 
002MIN		= 
002MAX		= 
002DECIMALS	= -2
002DIGITS	= 0
002LASTVAL	= 
003DESC		= Spindle speed units/min
003REQUIRED	= No
003ISFUNC	= No
003USESIGN	= No
003UPPERCASE	= Yes
003ALLOWNEG	= No
003NOEMPTYLINE	= No
003ALLOWALPHA	= No
003REMEBER	= Yes
003DEFAULT	= 
003PREFIX	= S
003SUFFIX	= 
003MIN		= 
003MAX		= 
003DECIMALS	= 0
003DIGITS	= 0
003LASTVAL	= 

## MACRO046 ###################################################################

[MACRO046]
NAME		= G71 Profile roughing cycle turning and boring
HIDEFORMULAS	= No
TEXT		= G71 $1 $2ÿG71 $3 $4 $5 $6 $7 $8
PARAMCOUNT	= 8
000DESC		= (U) Depth of roughing cut
000REQUIRED	= Yes
000ISFUNC	= No
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= No
000NOEMPTYLINE	= No
000ALLOWALPHA	= No
000REMEBER	= Yes
000DEFAULT	= 
000PREFIX	= U
000SUFFIX	= 
000MIN		= 
000MAX		= 
000DECIMALS	= -2
000DIGITS	= 0
000LASTVAL	= 1
001DESC		= (R) Amount of retract from each cut
001REQUIRED	= Yes
001ISFUNC	= No
001USESIGN	= No
001UPPERCASE	= Yes
001ALLOWNEG	= No
001NOEMPTYLINE	= No
001ALLOWALPHA	= No
001REMEBER	= Yes
001DEFAULT	= 
001PREFIX	= R
001SUFFIX	= 
001MIN		= 
001MAX		= 
001DECIMALS	= -2
001DIGITS	= 0
001LASTVAL	= 1.5
002DESC		= (P) First block number of of the finishing contour
002REQUIRED	= Yes
002ISFUNC	= No
002USESIGN	= No
002UPPERCASE	= Yes
002ALLOWNEG	= No
002NOEMPTYLINE	= No
002ALLOWALPHA	= No
002REMEBER	= Yes
002DEFAULT	= 
002PREFIX	= P
002SUFFIX	= 
002MIN		= 
002MAX		= 
002DECIMALS	= 0
002DIGITS	= 0
002LASTVAL	= 100
003DESC		= (Q) Last block number of the finishing contour
003REQUIRED	= Yes
003ISFUNC	= No
003USESIGN	= No
003UPPERCASE	= Yes
003ALLOWNEG	= No
003NOEMPTYLINE	= No
003ALLOWALPHA	= No
003REMEBER	= Yes
003DEFAULT	= 
003PREFIX	= Q
003SUFFIX	= 
003MIN		= 
003MAX		= 
003DECIMALS	= 0
003DIGITS	= 0
003LASTVAL	= 200
004DESC		= (U) Stock amount  for finishing on the X axis diameter
004REQUIRED	= Yes
004ISFUNC	= No
004USESIGN	= No
004UPPERCASE	= Yes
004ALLOWNEG	= No
004NOEMPTYLINE	= No
004ALLOWALPHA	= No
004REMEBER	= Yes
004DEFAULT	= 
004PREFIX	= U
004SUFFIX	= 
004MIN		= 
004MAX		= 
004DECIMALS	= -2
004DIGITS	= 0
004LASTVAL	= .5
005DESC		= (W) Stock left for finishing on the Z axis
005REQUIRED	= Yes
005ISFUNC	= No
005USESIGN	= No
005UPPERCASE	= Yes
005ALLOWNEG	= No
005NOEMPTYLINE	= No
005ALLOWALPHA	= No
005REMEBER	= Yes
005DEFAULT	= 
005PREFIX	= W
005SUFFIX	= 
005MIN		= 
005MAX		= 
005DECIMALS	= -2
005DIGITS	= 0
005LASTVAL	= .5
006DESC		= (F) Cutting feedrate units/rev overrides feedrates between P and Q block
006REQUIRED	= No
006ISFUNC	= No
006USESIGN	= No
006UPPERCASE	= Yes
006ALLOWNEG	= No
006NOEMPTYLINE	= No
006ALLOWALPHA	= No
006REMEBER	= Yes
006DEFAULT	= 
006PREFIX	= F
006SUFFIX	= 
006MIN		= 
006MAX		= 
006DECIMALS	= -2
006DIGITS	= 0
006LASTVAL	= 
007DESC		= (S) Spindle speed units/min overrides spindle speeds between P and Q blocks
007REQUIRED	= No
007ISFUNC	= No
007USESIGN	= No
007UPPERCASE	= Yes
007ALLOWNEG	= No
007NOEMPTYLINE	= No
007ALLOWALPHA	= No
007REMEBER	= Yes
007DEFAULT	= 
007PREFIX	= S
007SUFFIX	= 
007MIN		= 
007MAX		= 
007DECIMALS	= 0
007DIGITS	= 0
007LASTVAL	= 

## MACRO047 ###################################################################

[MACRO047]
NAME		= G72 Profile roughing cycle facing
HIDEFORMULAS	= No
TEXT		= G72
PARAMCOUNT	= 0

## MACRO048 ###################################################################

[MACRO048]
NAME		= G73 Pattern repeating
HIDEFORMULAS	= No
TEXT		= G73
PARAMCOUNT	= 0

## MACRO049 ###################################################################

[MACRO049]
NAME		= G74 Deep hole drilling in Z axis
HIDEFORMULAS	= No
TEXT		= G74
PARAMCOUNT	= 0

## MACRO050 ###################################################################

[MACRO050]
NAME		= G75 Grooving/Drilling  in X axis
HIDEFORMULAS	= No
TEXT		= G75
PARAMCOUNT	= 0

## MACRO051 ###################################################################

[MACRO051]
NAME		= G76 Multiple thread cutting cycle
HIDEFORMULAS	= No
TEXT		= G76
PARAMCOUNT	= 0

## MACRO052 ###################################################################

[MACRO052]
NAME		= G80 Cancel drill cycle
HIDEFORMULAS	= No
TEXT		= G80
PARAMCOUNT	= 0

## MACRO053 ###################################################################

[MACRO053]
NAME		= G83 Cycle for face drilling
HIDEFORMULAS	= No
TEXT		= G00 X0. $1ÿG83 $2 @5{$3-$1} $4ÿG80ÿ
PARAMCOUNT	= 5
000DESC		= Clearance Z
000REQUIRED	= Yes
000ISFUNC	= No
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= No
000NOEMPTYLINE	= No
000ALLOWALPHA	= No
000REMEBER	= No
000DEFAULT	= 
000PREFIX	= Z
000SUFFIX	= 
000MIN		= 
000MAX		= 
000DECIMALS	= -1
000DIGITS	= 0
000LASTVAL	= 10
001DESC		= Drill depth
001REQUIRED	= Yes
001ISFUNC	= No
001USESIGN	= No
001UPPERCASE	= Yes
001ALLOWNEG	= Yes
001NOEMPTYLINE	= No
001ALLOWALPHA	= No
001REMEBER	= Yes
001DEFAULT	= 
001PREFIX	= Z
001SUFFIX	= 
001MIN		= 
001MAX		= 
001DECIMALS	= -2
001DIGITS	= 0
001LASTVAL	= -5
002DESC		= Retract plane
002REQUIRED	= Yes
002ISFUNC	= No
002USESIGN	= No
002UPPERCASE	= Yes
002ALLOWNEG	= Yes
002NOEMPTYLINE	= No
002ALLOWALPHA	= No
002REMEBER	= Yes
002DEFAULT	= 
002PREFIX	= 
002SUFFIX	= 
002MIN		= 
002MAX		= 
002DECIMALS	= -2
002DIGITS	= 0
002LASTVAL	= 5
003DESC		= Feed rate (Check G98/G98)
003REQUIRED	= Yes
003ISFUNC	= No
003USESIGN	= No
003UPPERCASE	= Yes
003ALLOWNEG	= No
003NOEMPTYLINE	= No
003ALLOWALPHA	= No
003REMEBER	= Yes
003DEFAULT	= 
003PREFIX	= F
003SUFFIX	= 
003MIN		= 
003MAX		= 
003DECIMALS	= -2
003DIGITS	= 0
003LASTVAL	= .5
004DESC		= 
004REQUIRED	= No
004ISFUNC	= Yes
004USESIGN	= No
004UPPERCASE	= Yes
004ALLOWNEG	= Yes
004NOEMPTYLINE	= No
004ALLOWALPHA	= No
004REMEBER	= Yes
004DEFAULT	= 
004PREFIX	= R
004SUFFIX	= 
004MIN		= 
004MAX		= 
004DECIMALS	= -2
004DIGITS	= 0
004LASTVAL	= -5

## MACRO054 ###################################################################

[MACRO054]
NAME		= G84 Cycle for face tapping
HIDEFORMULAS	= No
TEXT		= G84 $1 $2 $3
PARAMCOUNT	= 3
000DESC		= Z depth (absolute)
000REQUIRED	= Yes
000ISFUNC	= No
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= Yes
000NOEMPTYLINE	= No
000ALLOWALPHA	= No
000REMEBER	= No
000DEFAULT	= 
000PREFIX	= Z
000SUFFIX	= 
000MIN		= 
000MAX		= 
000DECIMALS	= -1
000DIGITS	= 0
000LASTVAL	= 
001DESC		= R reference height (absolute)
001REQUIRED	= Yes
001ISFUNC	= No
001USESIGN	= No
001UPPERCASE	= Yes
001ALLOWNEG	= Yes
001NOEMPTYLINE	= No
001ALLOWALPHA	= No
001REMEBER	= Yes
001DEFAULT	= 
001PREFIX	= R
001SUFFIX	= 
001MIN		= 
001MAX		= 
001DECIMALS	= -1
001DIGITS	= 0
001LASTVAL	= 
002DESC		= E Thread pitch
002REQUIRED	= Yes
002ISFUNC	= No
002USESIGN	= No
002UPPERCASE	= Yes
002ALLOWNEG	= No
002NOEMPTYLINE	= No
002ALLOWALPHA	= No
002REMEBER	= Yes
002DEFAULT	= 
002PREFIX	= E
002SUFFIX	= 
002MIN		= 
002MAX		= 
002DECIMALS	= -1
002DIGITS	= 0
002LASTVAL	= 

## MACRO055 ###################################################################

[MACRO055]
NAME		= G86 Cycle for face boring
HIDEFORMULAS	= No
TEXT		= G86
PARAMCOUNT	= 0

## MACRO056 ###################################################################

[MACRO056]
NAME		= G87 Cycle for side drilling
HIDEFORMULAS	= No
TEXT		= G87
PARAMCOUNT	= 0

## MACRO057 ###################################################################

[MACRO057]
NAME		= G88 Cycle for side tapping
HIDEFORMULAS	= No
TEXT		= G88
PARAMCOUNT	= 0

## MACRO058 ###################################################################

[MACRO058]
NAME		= G89 Cycle for side boring
HIDEFORMULAS	= No
TEXT		= G89
PARAMCOUNT	= 0

## MACRO059 ###################################################################

[MACRO059]
NAME		= G90 Simple diameter cutting cycle
HIDEFORMULAS	= No
TEXT		= G90 $1 $2 $3
PARAMCOUNT	= 3
000DESC		= Diameter to be cut
000REQUIRED	= Yes
000ISFUNC	= No
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= No
000NOEMPTYLINE	= No
000ALLOWALPHA	= No
000REMEBER	= Yes
000DEFAULT	= 
000PREFIX	= X
000SUFFIX	= 
000MIN		= 
000MAX		= 
000DECIMALS	= -2
000DIGITS	= 0
000LASTVAL	= 10
001DESC		= End of cut in Z position
001REQUIRED	= Yes
001ISFUNC	= No
001USESIGN	= No
001UPPERCASE	= Yes
001ALLOWNEG	= Yes
001NOEMPTYLINE	= No
001ALLOWALPHA	= No
001REMEBER	= Yes
001DEFAULT	= 
001PREFIX	= Z
001SUFFIX	= 
001MIN		= 
001MAX		= 
001DECIMALS	= -2
001DIGITS	= 0
001LASTVAL	= -50
002DESC		= Cutting feedrate units/rev
002REQUIRED	= Yes
002ISFUNC	= No
002USESIGN	= No
002UPPERCASE	= Yes
002ALLOWNEG	= No
002NOEMPTYLINE	= No
002ALLOWALPHA	= No
002REMEBER	= Yes
002DEFAULT	= 
002PREFIX	= F
002SUFFIX	= 
002MIN		= 
002MAX		= 
002DECIMALS	= -2
002DIGITS	= 0
002LASTVAL	= .1

## MACRO060 ###################################################################

[MACRO060]
NAME		= G92 Simple thread cutting cycle
HIDEFORMULAS	= No
TEXT		= G92
PARAMCOUNT	= 0

## MACRO061 ###################################################################

[MACRO061]
NAME		= G94 Simple face cutting cycle
HIDEFORMULAS	= No
TEXT		= G94
PARAMCOUNT	= 0

## MACRO062 ###################################################################

[MACRO062]
NAME		= G96 Constant surface speed ON
HIDEFORMULAS	= No
TEXT		= G96 $1
PARAMCOUNT	= 1
000DESC		= Spindle speed (m/min)
000REQUIRED	= Yes
000ISFUNC	= No
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= No
000NOEMPTYLINE	= No
000ALLOWALPHA	= No
000REMEBER	= Yes
000DEFAULT	= 
000PREFIX	= S
000SUFFIX	= 
000MIN		= 
000MAX		= 
000DECIMALS	= 0
000DIGITS	= 0
000LASTVAL	= 

## MACRO063 ###################################################################

[MACRO063]
NAME		= G97 Constant surface speed OFF
HIDEFORMULAS	= No
TEXT		= G97 $1
PARAMCOUNT	= 1
000DESC		= Spindle speed (rev/min)
000REQUIRED	= Yes
000ISFUNC	= No
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= No
000NOEMPTYLINE	= No
000ALLOWALPHA	= No
000REMEBER	= Yes
000DEFAULT	= 
000PREFIX	= S
000SUFFIX	= 
000MIN		= 
000MAX		= 
000DECIMALS	= 0
000DIGITS	= 0
000LASTVAL	= 

## MACRO064 ###################################################################

[MACRO064]
NAME		= G98 Feed per minute
HIDEFORMULAS	= No
TEXT		= G98
PARAMCOUNT	= 0

## MACRO065 ###################################################################

[MACRO065]
NAME		= G99 Feed per rev
HIDEFORMULAS	= No
TEXT		= G99
PARAMCOUNT	= 0

## MACRO066 ###################################################################

[MACRO066]
NAME		= M00 Program stop
HIDEFORMULAS	= No
TEXT		= M00
PARAMCOUNT	= 0

## MACRO067 ###################################################################

[MACRO067]
NAME		= M01 Optional stop
HIDEFORMULAS	= No
TEXT		= M01
PARAMCOUNT	= 0

## MACRO068 ###################################################################

[MACRO068]
NAME		= M02 Program end
HIDEFORMULAS	= No
TEXT		= M02
PARAMCOUNT	= 0

## MACRO069 ###################################################################

[MACRO069]
NAME		= M03 Spindle start clockwise
HIDEFORMULAS	= No
TEXT		= M03
PARAMCOUNT	= 0

## MACRO070 ###################################################################

[MACRO070]
NAME		= M04 Spindle start counter-clockwise
HIDEFORMULAS	= No
TEXT		= M04
PARAMCOUNT	= 0

## MACRO071 ###################################################################

[MACRO071]
NAME		= M05 Spindle stop
HIDEFORMULAS	= No
TEXT		= M05
PARAMCOUNT	= 0

## MACRO072 ###################################################################

[MACRO072]
NAME		= M08 Coolant on
HIDEFORMULAS	= No
TEXT		= M08
PARAMCOUNT	= 0

## MACRO073 ###################################################################

[MACRO073]
NAME		= M09 Coolant off
HIDEFORMULAS	= No
TEXT		= M09
PARAMCOUNT	= 0

## MACRO074 ###################################################################

[MACRO074]
NAME		= M30 End program (rewind stop)
HIDEFORMULAS	= No
TEXT		= M30
PARAMCOUNT	= 0

## MACRO075 ###################################################################

[MACRO075]
NAME		= M41 Gear range  selection low gear
HIDEFORMULAS	= No
TEXT		= M41
PARAMCOUNT	= 0

## MACRO076 ###################################################################

[MACRO076]
NAME		= M42 Gear range selection medium gear 1
HIDEFORMULAS	= No
TEXT		= M42
PARAMCOUNT	= 0

## MACRO077 ###################################################################

[MACRO077]
NAME		= M43 Gear range selection medium gear 2
HIDEFORMULAS	= No
TEXT		= M43
PARAMCOUNT	= 0

## MACRO078 ###################################################################

[MACRO078]
NAME		= M44 Gear range selection high gear
HIDEFORMULAS	= No
TEXT		= M44
PARAMCOUNT	= 0

## MACRO079 ###################################################################

[MACRO079]
NAME		= M98 Subprogram call
HIDEFORMULAS	= No
TEXT		= M98
PARAMCOUNT	= 0

## MACRO080 ###################################################################

[MACRO080]
NAME		= M99 Subprogram end or Macro end
HIDEFORMULAS	= No
TEXT		= M99
PARAMCOUNT	= 0
