
## INIFILEVERSION #############################################################

[INIFILEVERSION]
VERSION		= 200

## GENERAL ####################################################################

[GENERAL]
DESCRIPTION	= ISO Milling
BASICTYPE	= 0
PRINTCOL	= 2
COLINDICATOR	= 60
HIDEASSIST	= No
LOADORDER	= 1

## RENUM ######################################################################

[RENUM]
AUTOINDENT	= Yes
UNDOLARGE	= No
INSERTSPACE	= 1
STARTNEXT	= No
RENUMEMPTY	= No
SHOWQUICK	= No
FORMAT		= 0
INTERVAL	= 1
START		= 100
FROM		= 0
TO		= 0
RESTART		= 0
RENUMCANNED	= No
PRECEEDESTR	= N
STARTTRIG	= 
SKIP		= %,O
SKIPCONTAIN	= 

## FILECOMPARE ################################################################

[FILECOMPARE]
SINGLESTEP	= Yes
IGNORECASE	= Yes
IGNOREBLOCK	= Yes
IGNORETNUMERIC	= Yes
IGNORECOMMENTS	= Yes
IGNOREWHITESPACE= Yes
MARKCHANGEONLY	= Yes
TABSWITCH	= Yes
SMARTMARK	= Yes
AUTONEXT	= Yes
SHOWALL		= Yes

## LOADSAVE ###################################################################

[LOADSAVE]
AUTOSAVETIME	= 0
LINEFEEDTYPE	= 0
DIFFLOADSAVE	= No
REGDEFAULTEXT	= Yes
REGOTHEREXT	= Yes
SAVEEXT		= NC
LOADEXT		= NCL,ISO,NCF
LOADPATH	= 
SAVEPATH	= 

## MACHINETYPE ################################################################

[MACHINETYPE]
BLOCKSKIP	= /
COMMENTSTART	= (
COMMENTEND	= )
DECIMAL		= .
FEED		= F
SPEED		= S
TOOLCHANGE	= T
TOOLLOAD	= M6
ARCTPYE		= 0
PATHUNIT	= 0
FEEDUNIT	= 0
BLOCKSKIPAFTER	= Yes
RAPIDRATE	= 1000

## BACKPLOT ###################################################################

[BACKPLOT]
TURNPRG		= No
DIAPRG		= Yes
DIAARC		= No
AUTOX		= Yes
SHOWCYCLES	= Yes
NULLARCS	= Yes
PRINTQUALITY	= 2
TOOLTYPE	= 0
PRINTLOWCOLOR	= Yes
PRINTNOWCOLOR	= No
PLOTMODE	= 2
DRAWDIMMED	= Yes
SHOWTOOL	= Yes
SHOWRAPIDMOVES	= Yes
SHOWDOTS	= No
SHOWVECTORS	= No
HIGHLIGHTARCS	= Yes
NOPERSPECTIVE	= No
HIDEPLOTCTRL	= No
HIDECOORD	= No
TOOLDIA		= 

## CNCCALC ####################################################################

[CNCCALC]
ISTURN		= No
DECIMALS	= 3
TURNNEGATIVEX	= No
TURNDIAMETERPRG	= Yes
TURNDIAMETERARC	= Yes
ARCTYPE		= 1
GRIDON		= Yes
AXISON		= Yes
MODALXY		= No
MODALZ		= Yes
ALWAYSSIGN	= No
SHOWSUBGRID	= Yes
GRIDSIZE	= 10.000000
TRAILZEROS	= 0
METRICIMPERIAL	= 0
MACROHEAD	= 
MACROTAIL	= 
DRAWDIR		= 

## NCBASE #####################################################################

[NCBASE]
GROUPS		= 
STORE		= No
ID		= 0

## MACROINF ###################################################################

[MACROINF]
COUNT		= 33
CURRENT		= 12

## COLORS #####################################################################

[COLORS]
USE		= 1
INBLOCK		= 1
USEMODALCOLORS	= 1
COUNT		= 30
COLOR0		= 0
COLOR1		= 16777215
COLOR2		= 65535
COLOR3		= 12582912
COLOR4		= 8388608
COLOR5		= 192
COLOR6		= 49152
COLOR7		= 12582912
COLOR8		= 12582912
COLOR9		= 16744576
COLOR19		= 255
COLOR10		= 16711935
COLOR11		= 0
COLOR12		= 8388736
COLOR13		= 8421504
COLOR14		= 16777215
COLOR15		= 65535
COLOR16		= 65535
COLOR17		= 3158064
COLOR18		= 8421504
COLOR20		= 0
COLOR21		= 16777215
COLOR22		= 12632256
COLOR23		= 11579568
COLOR24		= 57344
COLOR25		= 16777215
COLOR26		= 255
COLOR27		= 16711680
COLOR28		= 16777088
COLOR29		= 65535

## MACRO000 ###################################################################

[MACRO000]
NAME		= Program start
TEXT		= %ÿ$1ÿ(DATE: $DATETIME)ÿ(PROGRAMMER: $7)ÿ# G00 G40 G49 G80 G90ÿ# $2 M06ÿ# $3 M03ÿ# G00 $4 $5ÿ# G00 G43 $8 $6
PARAMCOUNT	= 8
000DESC		= O number
000REQUIRED	= Yes
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= No
000ALLOWALPHA	= No
000REMEBER	= No
000DEFAULT	= 
000PREFIX	= O
000SUFFIX	= 
000MIN		= 1000
000MAX		= 6999
000DECIMALS	= 0
000LASTVAL	= 
001DESC		= Tool number
001REQUIRED	= Yes
001USESIGN	= No
001UPPERCASE	= Yes
001ALLOWNEG	= No
001ALLOWALPHA	= No
001REMEBER	= No
001DEFAULT	= 
001PREFIX	= T
001SUFFIX	= 
001MIN		= 
001MAX		= 
001DECIMALS	= 0
001LASTVAL	= 
002DESC		= Spindle speed
002REQUIRED	= Yes
002USESIGN	= No
002UPPERCASE	= Yes
002ALLOWNEG	= No
002ALLOWALPHA	= No
002REMEBER	= No
002DEFAULT	= 
002PREFIX	= S
002SUFFIX	= 
002MIN		= 50
002MAX		= 60000
002DECIMALS	= 0
002LASTVAL	= 
003DESC		= X starting position
003REQUIRED	= Yes
003USESIGN	= No
003UPPERCASE	= Yes
003ALLOWNEG	= Yes
003ALLOWALPHA	= No
003REMEBER	= No
003DEFAULT	= 
003PREFIX	= X
003SUFFIX	= 
003MIN		= 
003MAX		= 
003DECIMALS	= -1
003LASTVAL	= 
004DESC		= Y starting position
004REQUIRED	= Yes
004USESIGN	= No
004UPPERCASE	= Yes
004ALLOWNEG	= Yes
004ALLOWALPHA	= No
004REMEBER	= No
004DEFAULT	= 
004PREFIX	= Y
004SUFFIX	= 
004MIN		= 
004MAX		= 
004DECIMALS	= -1
004LASTVAL	= 
005DESC		= Z starting position
005REQUIRED	= Yes
005USESIGN	= No
005UPPERCASE	= Yes
005ALLOWNEG	= Yes
005ALLOWALPHA	= No
005REMEBER	= No
005DEFAULT	= 
005PREFIX	= Z
005SUFFIX	= 
005MIN		= 
005MAX		= 
005DECIMALS	= -1
005LASTVAL	= 
006DESC		= Programmer name
006REQUIRED	= Yes
006USESIGN	= No
006UPPERCASE	= Yes
006ALLOWNEG	= Yes
006ALLOWALPHA	= Yes
006REMEBER	= Yes
006DEFAULT	= 
006PREFIX	= 
006SUFFIX	= 
006MIN		= 
006MAX		= 
006DECIMALS	= -1
006LASTVAL	= 
007DESC		= Tool length register
007REQUIRED	= Yes
007USESIGN	= No
007UPPERCASE	= Yes
007ALLOWNEG	= No
007ALLOWALPHA	= No
007REMEBER	= No
007DEFAULT	= 
007PREFIX	= H
007SUFFIX	= 
007MIN		= 
007MAX		= 
007DECIMALS	= 0
007LASTVAL	= 

## MACRO001 ###################################################################

[MACRO001]
NAME		= Tool change
TEXT		= ÿ# M05 M09ÿ# G00 G28 G91 Z0ÿ# G00 G90ÿ# $1 M06ÿ# $2 M03ÿ# G00 $3 $4ÿ# G00 G43 $6 $5
PARAMCOUNT	= 6
000DESC		= Tool number
000REQUIRED	= Yes
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= No
000ALLOWALPHA	= No
000REMEBER	= No
000DEFAULT	= 
000PREFIX	= T
000SUFFIX	= 
000MIN		= 
000MAX		= 
000DECIMALS	= 0
000LASTVAL	= 
001DESC		= Spindle speed
001REQUIRED	= Yes
001USESIGN	= No
001UPPERCASE	= Yes
001ALLOWNEG	= No
001ALLOWALPHA	= No
001REMEBER	= No
001DEFAULT	= 
001PREFIX	= S
001SUFFIX	= 
001MIN		= 50
001MAX		= 60000
001DECIMALS	= 0
001LASTVAL	= 
002DESC		= X starting position
002REQUIRED	= Yes
002USESIGN	= No
002UPPERCASE	= Yes
002ALLOWNEG	= Yes
002ALLOWALPHA	= No
002REMEBER	= No
002DEFAULT	= 
002PREFIX	= X
002SUFFIX	= 
002MIN		= 
002MAX		= 
002DECIMALS	= -1
002LASTVAL	= 
003DESC		= Y starting position
003REQUIRED	= Yes
003USESIGN	= No
003UPPERCASE	= Yes
003ALLOWNEG	= Yes
003ALLOWALPHA	= No
003REMEBER	= No
003DEFAULT	= 
003PREFIX	= Y
003SUFFIX	= 
003MIN		= 
003MAX		= 
003DECIMALS	= -1
003LASTVAL	= 
004DESC		= Z starting position
004REQUIRED	= Yes
004USESIGN	= No
004UPPERCASE	= Yes
004ALLOWNEG	= Yes
004ALLOWALPHA	= No
004REMEBER	= No
004DEFAULT	= 
004PREFIX	= Z
004SUFFIX	= 
004MIN		= 
004MAX		= 
004DECIMALS	= -1
004LASTVAL	= 
005DESC		= Tool length register
005REQUIRED	= Yes
005USESIGN	= No
005UPPERCASE	= Yes
005ALLOWNEG	= No
005ALLOWALPHA	= No
005REMEBER	= No
005DEFAULT	= 
005PREFIX	= H
005SUFFIX	= 
005MIN		= 
005MAX		= 
005DECIMALS	= 0
005LASTVAL	= 

## MACRO002 ###################################################################

[MACRO002]
NAME		= End of program
TEXT		= ÿ# M05 M09ÿ# G00 G28 G91 Z0ÿ# G00 G90ÿ# M30ÿ%
PARAMCOUNT	= 0

## MACRO003 ###################################################################

[MACRO003]
NAME		= Feed rate
TEXT		= $1
PARAMCOUNT	= 1
000DESC		= Feed rate
000REQUIRED	= Yes
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= No
000ALLOWALPHA	= No
000REMEBER	= Yes
000DEFAULT	= 
000PREFIX	= F
000SUFFIX	= 
000MIN		= 
000MAX		= 
000DECIMALS	= -1
000LASTVAL	= 

## MACRO004 ###################################################################

[MACRO004]
NAME		= G00 Rapid move
TEXT		= ÿ# G00 $1 $2 $3
PARAMCOUNT	= 3
000DESC		= X coordinate
000REQUIRED	= No
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= Yes
000ALLOWALPHA	= No
000REMEBER	= No
000DEFAULT	= 
000PREFIX	= X
000SUFFIX	= 
000MIN		= 
000MAX		= 
000DECIMALS	= -1
000LASTVAL	= 
001DESC		= Y Coordinate
001REQUIRED	= No
001USESIGN	= No
001UPPERCASE	= Yes
001ALLOWNEG	= Yes
001ALLOWALPHA	= No
001REMEBER	= No
001DEFAULT	= 
001PREFIX	= Y
001SUFFIX	= 
001MIN		= 
001MAX		= 
001DECIMALS	= -1
001LASTVAL	= 
002DESC		= Z coordinate
002REQUIRED	= No
002USESIGN	= No
002UPPERCASE	= Yes
002ALLOWNEG	= Yes
002ALLOWALPHA	= No
002REMEBER	= No
002DEFAULT	= 
002PREFIX	= Z
002SUFFIX	= 
002MIN		= 
002MAX		= 
002DECIMALS	= -1
002LASTVAL	= 

## MACRO005 ###################################################################

[MACRO005]
NAME		= G01 Linear move
TEXT		= ÿ# G01 $1 $2 $3
PARAMCOUNT	= 3
000DESC		= X coordinate
000REQUIRED	= No
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= Yes
000ALLOWALPHA	= No
000REMEBER	= No
000DEFAULT	= 
000PREFIX	= X
000SUFFIX	= 
000MIN		= 
000MAX		= 
000DECIMALS	= -1
000LASTVAL	= 
001DESC		= Y coordinate
001REQUIRED	= No
001USESIGN	= No
001UPPERCASE	= Yes
001ALLOWNEG	= Yes
001ALLOWALPHA	= No
001REMEBER	= No
001DEFAULT	= 
001PREFIX	= Y
001SUFFIX	= 
001MIN		= 
001MAX		= 
001DECIMALS	= -1
001LASTVAL	= 
002DESC		= Z coordinate
002REQUIRED	= No
002USESIGN	= No
002UPPERCASE	= Yes
002ALLOWNEG	= Yes
002ALLOWALPHA	= No
002REMEBER	= No
002DEFAULT	= 
002PREFIX	= Z
002SUFFIX	= 
002MIN		= 
002MAX		= 
002DECIMALS	= -1
002LASTVAL	= 

## MACRO006 ###################################################################

[MACRO006]
NAME		= G02 Clockwise arc move
TEXT		= ÿ# G02 $1 $2 $3 $4
PARAMCOUNT	= 4
000DESC		= X coordinate
000REQUIRED	= No
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= Yes
000ALLOWALPHA	= No
000REMEBER	= No
000DEFAULT	= 
000PREFIX	= X
000SUFFIX	= 
000MIN		= 
000MAX		= 
000DECIMALS	= -1
000LASTVAL	= 
001DESC		= Y coordinate
001REQUIRED	= No
001USESIGN	= No
001UPPERCASE	= Yes
001ALLOWNEG	= Yes
001ALLOWALPHA	= No
001REMEBER	= No
001DEFAULT	= 
001PREFIX	= Y
001SUFFIX	= 
001MIN		= 
001MAX		= 
001DECIMALS	= -1
001LASTVAL	= 
002DESC		= Z coordinate
002REQUIRED	= No
002USESIGN	= No
002UPPERCASE	= Yes
002ALLOWNEG	= Yes
002ALLOWALPHA	= No
002REMEBER	= No
002DEFAULT	= 
002PREFIX	= Z
002SUFFIX	= 
002MIN		= 
002MAX		= 
002DECIMALS	= -1
002LASTVAL	= 
003DESC		= Arc radius (set negative for arc sweep greater than 180 degrees)
003REQUIRED	= Yes
003USESIGN	= No
003UPPERCASE	= Yes
003ALLOWNEG	= Yes
003ALLOWALPHA	= No
003REMEBER	= Yes
003DEFAULT	= 
003PREFIX	= R
003SUFFIX	= 
003MIN		= 
003MAX		= 
003DECIMALS	= -1
003LASTVAL	= 

## MACRO007 ###################################################################

[MACRO007]
NAME		= G03 Counterclockwise arc move
TEXT		= ÿ# G03 $1 $2 $3 $4
PARAMCOUNT	= 4
000DESC		= X coordinate
000REQUIRED	= No
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= Yes
000ALLOWALPHA	= No
000REMEBER	= No
000DEFAULT	= 
000PREFIX	= X
000SUFFIX	= 
000MIN		= 
000MAX		= 
000DECIMALS	= -1
000LASTVAL	= 
001DESC		= Y coordinate
001REQUIRED	= No
001USESIGN	= No
001UPPERCASE	= Yes
001ALLOWNEG	= Yes
001ALLOWALPHA	= No
001REMEBER	= No
001DEFAULT	= 
001PREFIX	= Y
001SUFFIX	= 
001MIN		= 
001MAX		= 
001DECIMALS	= -1
001LASTVAL	= 
002DESC		= Z coordinate
002REQUIRED	= No
002USESIGN	= No
002UPPERCASE	= Yes
002ALLOWNEG	= Yes
002ALLOWALPHA	= No
002REMEBER	= No
002DEFAULT	= 
002PREFIX	= Z
002SUFFIX	= 
002MIN		= 
002MAX		= 
002DECIMALS	= -1
002LASTVAL	= 
003DESC		= Arc radius (set negative for arc sweep greater than 180 degrees)
003REQUIRED	= Yes
003USESIGN	= No
003UPPERCASE	= Yes
003ALLOWNEG	= Yes
003ALLOWALPHA	= No
003REMEBER	= Yes
003DEFAULT	= 
003PREFIX	= R
003SUFFIX	= 
003MIN		= 
003MAX		= 
003DECIMALS	= -1
003LASTVAL	= 

## MACRO008 ###################################################################

[MACRO008]
NAME		= G04 Dwell
TEXT		= ÿ# G04 $1
PARAMCOUNT	= 1
000DESC		= Dwell time (seconds)
000REQUIRED	= Yes
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= No
000ALLOWALPHA	= No
000REMEBER	= Yes
000DEFAULT	= 
000PREFIX	= X
000SUFFIX	= 
000MIN		= 
000MAX		= 
000DECIMALS	= -1
000LASTVAL	= 

## MACRO009 ###################################################################

[MACRO009]
NAME		= G17 XY plane specification
TEXT		= G17
PARAMCOUNT	= 0

## MACRO010 ###################################################################

[MACRO010]
NAME		= G18 XZ plane specification
TEXT		= G18
PARAMCOUNT	= 0

## MACRO011 ###################################################################

[MACRO011]
NAME		= G19 YZ plane specification
TEXT		= G19
PARAMCOUNT	= 0

## MACRO012 ###################################################################

[MACRO012]
NAME		= G28 Machine coordinate mode
TEXT		= G28
PARAMCOUNT	= 0

## MACRO013 ###################################################################

[MACRO013]
NAME		= G40 Radius compensation off
TEXT		= G40
PARAMCOUNT	= 0

## MACRO014 ###################################################################

[MACRO014]
NAME		= G41 Radius compensation, left
TEXT		= G41 $1
PARAMCOUNT	= 1
000DESC		= Tool diameter register
000REQUIRED	= Yes
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= No
000ALLOWALPHA	= No
000REMEBER	= Yes
000DEFAULT	= 
000PREFIX	= D
000SUFFIX	= 
000MIN		= 
000MAX		= 
000DECIMALS	= 0
000LASTVAL	= 

## MACRO015 ###################################################################

[MACRO015]
NAME		= G42 Radius compensation, right
TEXT		= G42 $1
PARAMCOUNT	= 1
000DESC		= Tool diameter register
000REQUIRED	= Yes
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= No
000ALLOWALPHA	= No
000REMEBER	= Yes
000DEFAULT	= 
000PREFIX	= D
000SUFFIX	= 
000MIN		= 
000MAX		= 
000DECIMALS	= 0
000LASTVAL	= 

## MACRO016 ###################################################################

[MACRO016]
NAME		= G43 Tool length compensation
TEXT		= G43 $1
PARAMCOUNT	= 1
000DESC		= Tool length register
000REQUIRED	= Yes
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= No
000ALLOWALPHA	= No
000REMEBER	= No
000DEFAULT	= 
000PREFIX	= H
000SUFFIX	= 
000MIN		= 
000MAX		= 
000DECIMALS	= 0
000LASTVAL	= 

## MACRO017 ###################################################################

[MACRO017]
NAME		= G49 Tool length compensation off
TEXT		= G49
PARAMCOUNT	= 0

## MACRO018 ###################################################################

[MACRO018]
NAME		= G81 Drilling
TEXT		= ÿ# G81 $1 $2 $3 $4 $5 $6
PARAMCOUNT	= 6
000DESC		= X coordinate
000REQUIRED	= No
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= Yes
000ALLOWALPHA	= No
000REMEBER	= No
000DEFAULT	= 
000PREFIX	= X
000SUFFIX	= 
000MIN		= 
000MAX		= 
000DECIMALS	= -1
000LASTVAL	= 
001DESC		= Y coordinate
001REQUIRED	= No
001USESIGN	= No
001UPPERCASE	= Yes
001ALLOWNEG	= Yes
001ALLOWALPHA	= No
001REMEBER	= No
001DEFAULT	= 
001PREFIX	= Y
001SUFFIX	= 
001MIN		= 
001MAX		= 
001DECIMALS	= -1
001LASTVAL	= 
002DESC		= Z depth (absolute)
002REQUIRED	= Yes
002USESIGN	= No
002UPPERCASE	= Yes
002ALLOWNEG	= Yes
002ALLOWALPHA	= No
002REMEBER	= No
002DEFAULT	= 
002PREFIX	= Z
002SUFFIX	= 
002MIN		= 
002MAX		= 
002DECIMALS	= -1
002LASTVAL	= 
003DESC		= R reference height (absolute)
003REQUIRED	= Yes
003USESIGN	= No
003UPPERCASE	= Yes
003ALLOWNEG	= Yes
003ALLOWALPHA	= No
003REMEBER	= Yes
003DEFAULT	= 
003PREFIX	= R
003SUFFIX	= 
003MIN		= 
003MAX		= 
003DECIMALS	= -1
003LASTVAL	= 
004DESC		= P dwell time (seconds)
004REQUIRED	= No
004USESIGN	= No
004UPPERCASE	= Yes
004ALLOWNEG	= No
004ALLOWALPHA	= No
004REMEBER	= Yes
004DEFAULT	= 
004PREFIX	= P
004SUFFIX	= 
004MIN		= 
004MAX		= 
004DECIMALS	= -1
004LASTVAL	= 
005DESC		= Feed rate
005REQUIRED	= Yes
005USESIGN	= No
005UPPERCASE	= Yes
005ALLOWNEG	= No
005ALLOWALPHA	= No
005REMEBER	= Yes
005DEFAULT	= 
005PREFIX	= F
005SUFFIX	= 
005MIN		= 
005MAX		= 
005DECIMALS	= -1
005LASTVAL	= 

## MACRO019 ###################################################################

[MACRO019]
NAME		= G82 Peck drilling
TEXT		= ÿ# G82 $1 $2 $3 $4 $6 $5 $7
PARAMCOUNT	= 7
000DESC		= X coordinate
000REQUIRED	= No
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= Yes
000ALLOWALPHA	= No
000REMEBER	= No
000DEFAULT	= 
000PREFIX	= X
000SUFFIX	= 
000MIN		= 
000MAX		= 
000DECIMALS	= -1
000LASTVAL	= 
001DESC		= Y coordinate
001REQUIRED	= No
001USESIGN	= No
001UPPERCASE	= Yes
001ALLOWNEG	= Yes
001ALLOWALPHA	= No
001REMEBER	= No
001DEFAULT	= 
001PREFIX	= Y
001SUFFIX	= 
001MIN		= 
001MAX		= 
001DECIMALS	= -1
001LASTVAL	= 
002DESC		= Z depth (absolute)
002REQUIRED	= Yes
002USESIGN	= No
002UPPERCASE	= Yes
002ALLOWNEG	= Yes
002ALLOWALPHA	= No
002REMEBER	= No
002DEFAULT	= 
002PREFIX	= Z
002SUFFIX	= 
002MIN		= 
002MAX		= 
002DECIMALS	= -1
002LASTVAL	= 
003DESC		= R reference height (absolute)
003REQUIRED	= Yes
003USESIGN	= No
003UPPERCASE	= Yes
003ALLOWNEG	= Yes
003ALLOWALPHA	= No
003REMEBER	= Yes
003DEFAULT	= 
003PREFIX	= R
003SUFFIX	= 
003MIN		= 
003MAX		= 
003DECIMALS	= -1
003LASTVAL	= 
004DESC		= P dwell time (seconds)
004REQUIRED	= No
004USESIGN	= No
004UPPERCASE	= Yes
004ALLOWNEG	= No
004ALLOWALPHA	= No
004REMEBER	= Yes
004DEFAULT	= 
004PREFIX	= P
004SUFFIX	= 
004MIN		= 
004MAX		= 
004DECIMALS	= -1
004LASTVAL	= 
005DESC		= Q peck step
005REQUIRED	= No
005USESIGN	= No
005UPPERCASE	= Yes
005ALLOWNEG	= No
005ALLOWALPHA	= No
005REMEBER	= Yes
005DEFAULT	= 
005PREFIX	= Q
005SUFFIX	= 
005MIN		= 
005MAX		= 
005DECIMALS	= -1
005LASTVAL	= 
006DESC		= Feed rate
006REQUIRED	= Yes
006USESIGN	= No
006UPPERCASE	= Yes
006ALLOWNEG	= No
006ALLOWALPHA	= No
006REMEBER	= Yes
006DEFAULT	= 
006PREFIX	= F
006SUFFIX	= 
006MIN		= 
006MAX		= 
006DECIMALS	= -1
006LASTVAL	= 

## MACRO020 ###################################################################

[MACRO020]
NAME		= G84 Tapping
TEXT		= ÿ# G84 $1 $2 $3 $4 $5
PARAMCOUNT	= 5
000DESC		= X coordinate
000REQUIRED	= No
000USESIGN	= No
000UPPERCASE	= Yes
000ALLOWNEG	= Yes
000ALLOWALPHA	= No
000REMEBER	= No
000DEFAULT	= 
000PREFIX	= X
000SUFFIX	= 
000MIN		= 
000MAX		= 
000DECIMALS	= -1
000LASTVAL	= 
001DESC		= Y coordinate
001REQUIRED	= No
001USESIGN	= No
001UPPERCASE	= Yes
001ALLOWNEG	= Yes
001ALLOWALPHA	= No
001REMEBER	= No
001DEFAULT	= 
001PREFIX	= Y
001SUFFIX	= 
001MIN		= 
001MAX		= 
001DECIMALS	= -1
001LASTVAL	= 
002DESC		= Z depth (absolute)
002REQUIRED	= Yes
002USESIGN	= No
002UPPERCASE	= Yes
002ALLOWNEG	= Yes
002ALLOWALPHA	= No
002REMEBER	= No
002DEFAULT	= 
002PREFIX	= Z
002SUFFIX	= 
002MIN		= 
002MAX		= 
002DECIMALS	= -1
002LASTVAL	= 
003DESC		= R reference height (absolute)
003REQUIRED	= Yes
003USESIGN	= No
003UPPERCASE	= Yes
003ALLOWNEG	= Yes
003ALLOWALPHA	= No
003REMEBER	= Yes
003DEFAULT	= 
003PREFIX	= R
003SUFFIX	= 
003MIN		= 
003MAX		= 
003DECIMALS	= -1
003LASTVAL	= 
004DESC		= E Thread pitch
004REQUIRED	= Yes
004USESIGN	= No
004UPPERCASE	= Yes
004ALLOWNEG	= No
004ALLOWALPHA	= No
004REMEBER	= Yes
004DEFAULT	= 
004PREFIX	= E
004SUFFIX	= 
004MIN		= 
004MAX		= 
004DECIMALS	= -1
004LASTVAL	= 

## MACRO021 ###################################################################

[MACRO021]
NAME		= G80 Cancel drill cycle
TEXT		= ÿ# G80
PARAMCOUNT	= 0

## MACRO022 ###################################################################

[MACRO022]
NAME		= G90 Absolute coordinates mode
TEXT		= G90
PARAMCOUNT	= 0

## MACRO023 ###################################################################

[MACRO023]
NAME		= G91 Incremental coordinates mode
TEXT		= G91
PARAMCOUNT	= 0

## MACRO024 ###################################################################

[MACRO024]
NAME		= M00 Program stop
TEXT		= ÿ# M00
PARAMCOUNT	= 0

## MACRO025 ###################################################################

[MACRO025]
NAME		= M01 Optional stop
TEXT		= ÿ# M01
PARAMCOUNT	= 0

## MACRO026 ###################################################################

[MACRO026]
NAME		= M02 Program end
TEXT		= ÿ# M02
PARAMCOUNT	= 0

## MACRO027 ###################################################################

[MACRO027]
NAME		= M03 Spindle start clockwise
TEXT		= M03
PARAMCOUNT	= 0

## MACRO028 ###################################################################

[MACRO028]
NAME		= M04 Spindle start counter-clockwise
TEXT		= M04
PARAMCOUNT	= 0

## MACRO029 ###################################################################

[MACRO029]
NAME		= M05 Spindle stop
TEXT		= ÿ# M05
PARAMCOUNT	= 0

## MACRO030 ###################################################################

[MACRO030]
NAME		= M08 Coolant on
TEXT		= M08
PARAMCOUNT	= 0

## MACRO031 ###################################################################

[MACRO031]
NAME		= M09 Coolant off
TEXT		= M09
PARAMCOUNT	= 0

## MACRO032 ###################################################################

[MACRO032]
NAME		= M30 Program end with spindle and coolant stop and tape rewind
TEXT		= ÿ# M30
PARAMCOUNT	= 0
