<?xml version="1.0" encoding="gb2312" standalone="yes" ?>
<Channels>
    <Channel type="OPC" name="OPC" use="1" />
    <Channel type="以太网口" name="远动" use="0" cdt="1" freshtime="200" port="2404" IP="192.168.202.239" localPort="502" Mode="0" port2="502" IP2="" Double="0">
        <Device type="IEC104" name="长园深瑞" use="1" address="1" alarm="0" notes="IEC104远端为TCP Server，端口号2404" param="" ChuansongyuanyinLen="2" GonggongdizhiLen="2" XinxidizhiLen="3" T0="30" T1="15" T2="10" T3="20" Zongzhao="1" Diandu="1" Jiaoshi="0" ZongzhaoZhouqi="120" Dianduzhouqi="300" JiaoshiZhouqi="30">
            <DataBlock type="YX" name="YX" length="1188" address="0" />
            <DataBlock type="YC" name="YC" length="3880" address="0" />
            <DataBlock type="DD" name="DD" length="1764" address="0" />
        </Device>
    </Channel>
</Channels>
